**External grille LZP-R 31**

Weather protection grille for ventilation and air extraction constructed to very high quality standard.

With channel cross-section extension as standard to reduce pressure losses.

With fixed rain-repellent weather protection lamella.

With frame for mounting in masonry walls.

With 20 mm flange frame and slots for direct connection with channel.

Protective grille in accordance with DIN EN ISO 13857.

Technical data

|  |  |
| --- | --- |
| Article: | LZP-R 31 |
| Air direction: | Ventilation and air extraction |
| Installation: | outside |
| Installation site: | Wall / Channel |
| Material: | Sheet steel, galvanised |
| Weight: | 17,4 kg |
| Weight including packaging: | 19,2 kg |
| Channel dimension: | 600 mm x 350 mm |
| Open cross section: | 1.701 cm² |
| Width: | 929 mm |
| Height: | 425 mm |
| Depth: | 250 mm |
| Width with packaging: | 1.005 mm |
| Height with packaging: | 430 mm |
| Depth with packaging: | 310 mm |
| Packing unit: | 1 piece |
| Range: | D |
| GTIN (EAN): | 4012799513841 |
| Article number: | 0151.0384 |

Manufacturer: MAICO

LZP-R 31 External grille