**Shutter, electric MK 20**

Electrical shutter for weather protection and prevention of cold air entry when fan is switched off.

MK with gear motor: Rated power 3 W, nominal current 0.015 A.

BK with bimetal cap: Rated power 25 W, rated current 0.01 A, start-up current 1.8 A - 1s. Speed control only with STU 2,5 / ST 2,5 speed controller.

Installation in accordance with protection class II (without protective-conductor terminal).

Opens and closes when the fan is switched on and off.

MK needs 4-core mains cable.

BK needs 3-core mains cable.

Special models with limit switch can be supplied on request. Limit switch is activated when the shutter is completely open.

Technical data

|  |  |
| --- | --- |
| Article: | MK 20 |
| Loss of pressure: | 11 Pa |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Frequency: | 50 Hz |
| Nominal output: | 3 W |
| Inom: | 0,015 A |
| Maximum load: | 0,015 A |
| Degree of protection: | IP 55 |
| Drive: | Gear |
| Installation: | outside |
| Installation site: | Wall |
| Installation position: | vertical |
| Material: | Synthetic material |
| Colour: | Traffic white, similar to RAL 9016 |
| Lamella colour: | Silver grey |
| Weight: | 1,16 kg |
| Weight including packaging: | 1,32 kg |
| Type of shutter: | electrical |
| Suitable for nominal size: | 200 mm |
| Width: | 325 mm |
| Height: | 325 mm |
| Depth: | 50,5 mm |
| Width with packaging: | 335 mm |
| Height with packaging: | 330 mm |
| Depth with packaging: | 60 mm |
| Ambient temperature: | 40 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799939061 |
| Article number: | 0093.0906 |

Manufacturer: MAICO

MK 20 Shutter, electric