**Shutter AS 35**

Shutters for air extraction.

With galvanised protective grille.

From nominal size 35 with centre bridge for increasing the stability of the shutters.

Recommended accessories: ZVR connection frames for mounting the AS and RS shutters to the fan rather than the wall.

Technical data

|  |  |
| --- | --- |
| Article: | AS 35 |
| Air direction: | Air extraction |
| Installation: | outside |
| Installation site: | Wall |
| Installation position: | vertical / horizontal |
| Material: | Synthetic material, weather and UV resistant |
| Colour: | Traffic white, similar to RAL 9016 |
| Lamella colour: | Silver grey |
| Weight: | 1,12 kg |
| Weight including packaging: | 1,36 kg |
| Type of shutter: | Airstream-operated opening/closing |
| Nominal size: | 355 mm |
| Width: | 360 mm |
| Height: | 360 mm |
| Depth: | 40 mm |
| Width with packaging: | 485 mm |
| Height with packaging: | 435 mm |
| Depth with packaging: | 50 mm |
| Ambient temperature: | 60 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799513339 |
| Article number: | 0151.0333 |

Manufacturer: MAICO

AS 35 Shutter