**Shutter, manual RS 45**

Shutters for air extraction and ventilation.

Lamella can be operated manually or with an additional MS 2 servomotor.

From nominal size 35 with centre bridge for increasing the stability of the shutters.

With pulley, 2.5 m pull cord and pull-cord clip.

With galvanised protective grille.

Recommended accessories: ZVR connection frames for mounting the AS and RS shutters to the fan rather than the wall.

Technical data

|  |  |
| --- | --- |
| Article: | RS 45 |
| Air direction: | Ventilation and air extraction |
| Installation: | outside |
| Installation site: | Wall |
| Installation position: | vertical |
| Material: | Synthetic material, weather and UV resistant |
| Colour: | Traffic white, similar to RAL 9016 |
| Lamella colour: | Silver grey |
| Weight: | 2,25 kg |
| Weight including packaging: | 2,63 kg |
| Type of shutter: | electrical / manual |
| Nominal size: | 450 mm |
| Width: | 526 mm |
| Height: | 526 mm |
| Depth: | 41 mm |
| Width with packaging: | 590 mm |
| Height with packaging: | 540 mm |
| Depth with packaging: | 50 mm |
| Ambient temperature: | 60 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799513438 |
| Article number: | 0151.0343 |

Manufacturer: MAICO

RS 45 Shutter, manual