**Shutter ARP 100**

Shutters for air extraction.

With individually moving lamella, fitted using reinforced bushing.

With galvanised protective grille on the inflow side.

Two-part ARP 71.

Three-part ARP 80 and ARP 100.

Technical data

|  |  |
| --- | --- |
| Article: | ARP 100 |
| Air direction: | Air extraction |
| Installation: | outside |
| Installation site: | Wall |
| Installation position: | vertical / horizontal |
| Material: | Synthetic material, weather and UV resistant |
| Colour: | Silver grey |
| Weight: | 7,5 kg |
| Weight including packaging: | 13,06 kg |
| Type of shutter: | Airstream-operated opening/closing |
| Suitable for nominal size: | 1.000 mm |
| Width: | 1.068 mm |
| Height: | 1.140 mm |
| Depth: | 40 mm |
| Width with packaging: | 1.180 mm |
| Height with packaging: | 1.180 mm |
| Depth with packaging: | 70 mm |
| Ambient temperature: | 60 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799510802 |
| Article number: | 0151.0080 |

Manufacturer: MAICO

ARP 100 Shutter