**Shutter, servomotor VE 40**

Shutters for automatic activation.

Must be combined with additional MS 8 or MS 8 P servomotors (servomotor is not included in the delivery).

Do not use in areas subject to explosions.

Installation instructions

Ensure access to the servomotor.

If required, fit an intermediate piece.

Technical data

|  |  |
| --- | --- |
| Article: | VE 40 |
| Material: | Sheet steel |
| Weight: | 6,7 kg |
| Weight including packaging: | 6,7 kg |
| Type of shutter: | electrical |
| Suitable for nominal size: | 400 mm |
| Width with packaging: | 465 mm |
| Height with packaging: | 425 mm |
| Depth with packaging: | 495 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799932888 |
| Article number: | 0093.0288 |

Manufacturer: MAICO

VE 40 Shutter, servomotor