**Shutter, servomotor VE 60**

Shutters for automatic activation.

Must be combined with additional MS 8 or MS 8 P servomotors (servomotor is not included in the delivery).

Do not use in areas subject to explosions.

Installation instructions

Ensure access to the servomotor.

If required, fit an intermediate piece.

Technical data

|  |  |
| --- | --- |
| Article: | VE 60 |
| Material: | Sheet steel |
| Weight: | 19,78 kg |
| Weight including packaging: | 19,8 kg |
| Type of shutter: | electrical |
| Suitable for nominal size: | 600 mm |
| Width: | 710 mm |
| Height: | 710 mm |
| Depth: | 620 mm |
| Width with packaging: | 710 mm |
| Height with packaging: | 710 mm |
| Depth with packaging: | 620 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799932901 |
| Article number: | 0093.0290 |

Manufacturer: MAICO

VE 60 Shutter, servomotor