**Channel shutter RKP 56**

With counter-rotating, hollow body lamella, which can be adjusted together over 15 x 15 mm square.

With U-shaped frame and flange holes on both sides.

With position indicator - Open/Closed.

Must be combined with additional MS 8 or MS 8 P servomotors (servomotor is not included in the delivery).

Technical data

|  |  |
| --- | --- |
| Article: | RKP 56 |
| Air direction: | Ventilation and air extraction |
| Installation site: | Channel |
| Installation position: | vertical / horizontal |
| Material: | Sheet steel, galvanised |
| Weight: | 11,77 kg |
| Weight including packaging: | 12,24 kg |
| Type of shutter: | electrical |
| Channel dimension: | 1.000 mm x 500 mm |
| Width: | 1.040 mm |
| Height: | 540 mm |
| Depth: | 120 mm |
| Width with packaging: | 1.140 mm |
| Height with packaging: | 540 mm |
| Depth with packaging: | 130 mm |
| Packing unit: | 1 piece |
| Range: | D |
| GTIN (EAN): | 4012799512417 |
| Article number: | 0151.0241 |

Manufacturer: MAICO

RKP 56 Channel shutter