**Automatic backflow preventer AVM 40**

Horizontal and vertical mounting is possible. Air flow direction for a vertical installation is from the bottom flowing upwards.

With 2 opposing shutter sections made of aluminium.

With wrap-around seal.

The backflow preventers are opened in the air flow and closed by spring force.

Technical data

|  |  |
| --- | --- |
| Article: | AVM 40 |
| Air direction: | Ventilation or air extraction |
| Installation position: | vertical / horizontal |
| Material: | Sheet steel, galvanised |
| Weight: | 2,6 kg |
| Weight including packaging: | 2,63 kg |
| Type of shutter: | Airstream-operated opening/closing |
| Nominal size: | 400 mm |
| Width: | 398 mm |
| Height: | 398 mm |
| Depth: | 198 mm |
| Width with packaging: | 398 mm |
| Height with packaging: | 398 mm |
| Depth with packaging: | 198 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799930136 |
| Article number: | 0093.0013 |

Manufacturer: MAICO

AVM 40 Automatic backflow preventer