**External grille SG 15**

External grille for ventilation and air extraction.

Exterior wall connection when using WH wall sleeve.

With galvanized protective grille.

With covered screw holes.

Sealing strip included in the scope of delivery.

Accessories: FG fly screen can be used.

External grille for ventilation and air extraction.

Exterior wall connection when using WH wall sleeve.

With covered screw holes.

Sealing strip included in the scope of delivery.

Accessories: FG fly screen can be used.

SG 120: Air filter retrofittable, SF 120.

Technical data

|  |  |
| --- | --- |
| Article: | SG 15 |
| Air direction: | Ventilation and air extraction |
| Installation: | outside |
| Installation site: | Wall |
| Type of installation: | Surface-mounted |
| Material: | Synthetic material, weather and UV resistant |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 0,23 kg |
| Weight including packaging: | 0,23 kg |
| Suitable for nominal size: | 150 mm |
| Width: | 200 mm |
| Height: | 200 mm |
| Depth: | 50 mm |
| Width with packaging: | 201 mm |
| Height with packaging: | 201 mm |
| Depth with packaging: | 51 mm |
| Ambient temperature: | 60 °C |
| Packing unit: | 1 piece |
| Range: | A |
| GTIN (EAN): | 4012799599043 |
| Article number: | 0059.0904 |

Manufacturer: MAICO

SG 15 External grille