**External grille MLZ 30**

External grille for ventilation and air extraction.

With fixed, rain-repellent weather protection lamellae.

With protective grille and mounting frame at the rear.

With integrated small animal guard.

Technical data

|  |  |
| --- | --- |
| Article: | MLZ 30 |
| Air direction: | Ventilation and air extraction |
| Max. flow velocity: | 4 m/s |
| Installation: | outside |
| Installation site: | Wall |
| Material: | Sheet steel, galvanised |
| Weight: | 2,43 kg |
| Weight including packaging: | 2,64 kg |
| Suitable for nominal size: | 300 mm |
| Open cross section: | 580 cm² |
| Width: | 357 mm |
| Height: | 330 mm |
| Depth: | 52 mm |
| Width with packaging: | 385 mm |
| Height with packaging: | 385 mm |
| Depth with packaging: | 60 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799511038 |
| Article number: | 0151.0103 |

Manufacturer: MAICO

MLZ 30 External grille