**External grille LAP 31**

External grille for air extraction and ventilation.

With fixed rain-repellent weather protection lamella.

With frame for mounting in masonry walls.

Protective grille in accordance with DIN EN ISO 13857.

Technical data

|  |  |
| --- | --- |
| Article: | LAP 31 |
| Air direction: | Ventilation and air extraction |
| Installation: | outside |
| Installation site: | Wall / Channel |
| Material: | Aluminium |
| Colour: | Anodised aluminium |
| Weight: | 5,9 kg |
| Weight including packaging: | 6,42 kg |
| Channel dimension: | 600 mm x 350 mm |
| Width: | 629 mm |
| Height: | 425 mm |
| Depth: | 73 mm |
| Width with packaging: | 710 mm |
| Height with packaging: | 435 mm |
| Depth with packaging: | 100 mm |
| Packing unit: | 1 piece |
| Range: | D |
| GTIN (EAN): | 4012799512530 |
| Article number: | 0151.0253 |

Manufacturer: MAICO

LAP 31 External grille