**External grille LZP 22**

External grille for air extraction and ventilation.

With fixed rain-repellent weather protection lamella.

With frame for mounting in masonry walls.

Protective grille in accordance with DIN EN ISO 13857.

Technical data

|  |  |
| --- | --- |
| Article: | LZP 22 |
| Air direction: | Ventilation and air extraction |
| Installation: | outside |
| Installation site: | Wall / Channel |
| Material: | Sheet steel, galvanised |
| Weight: | 6,45 kg |
| Weight including packaging: | 6,83 kg |
| Channel dimension: | 500 mm x 250 mm |
| Width: | 529 mm |
| Height: | 325 mm |
| Depth: | 73 mm |
| Width with packaging: | 590 mm |
| Height with packaging: | 335 mm |
| Depth with packaging: | 110 mm |
| Packing unit: | 1 piece |
| Range: | D |
| GTIN (EAN): | 4012799512554 |
| Article number: | 0151.0255 |

Manufacturer: MAICO

LZP 22 External grille