**Internal grille ESG 10/2**

Internal grille for ventilation and air extraction.

With air filter.

With covered screw holes.

Cover can be removed without tools for cleaning.

Sealing tape included in the scope of delivery.

Accessories: ZRF.. spare air filter.

Technical data

|  |  |
| --- | --- |
| Article: | ESG 10/2 |
| Air direction: | Ventilation and air extraction |
| Installation: | Inside |
| Installation site: | Wall |
| Type of installation: | Surface-mounted |
| Material: | Synthetic material |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 0,12 kg |
| Weight including packaging: | 0,13 kg |
| Filter class: | ISO Coarse 30 % (G2) |
| Suitable for nominal size: | 100 mm |
| Width: | 150 mm |
| Height: | 150 mm |
| Depth: | 51,5 mm |
| Width with packaging: | 151 mm |
| Height with packaging: | 151 mm |
| Depth with packaging: | 60 mm |
| Ambient temperature: | 60 °C |
| Packing unit: | 1 piece |
| Range: | A |
| GTIN (EAN): | 4012799599470 |
| Article number: | 0059.0947 |

Manufacturer: MAICO

ESG 10/2 Internal grille