**Internal shutter, electric AE 10**

Internal shutters for ventilation and air extraction.

Regulation of the air flow through adjustable opening and closing angle.

Heat energy saving by opening as required.

Control with commercially available circuit breakers, time switches and time delay relays.

With operating indicator light.

Technical data

|  |  |
| --- | --- |
| Article: | AE 10 |
| Air direction: | Ventilation and air extraction |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Frequency: | 50 Hz |
| Power consumption: | 10 W |
| Imax: | 0,04 A |
| Degree of protection: | IP 20 |
| Installation: | Inside |
| Installation site: | Wall / Ceiling |
| Installation position: | vertical / horizontal |
| Material: | Synthetic material |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 0,2 kg |
| Weight including packaging: | 0,266 kg |
| Type of shutter: | electrical |
| Suitable for nominal size: | 100 mm |
| Width: | 146 mm |
| Height: | 146 mm |
| Depth: | 60 mm |
| Width with packaging: | 175 mm |
| Height with packaging: | 150 mm |
| Depth with packaging: | 80 mm |
| Ambient temperature: | 40 °C |
| Packing unit: | 1 piece |
| Range: | A |
| GTIN (EAN): | 4012799513001 |
| Article number: | 0151.0300 |

Manufacturer: MAICO

AE 10 Internal shutter, electric