**Internal grille IG 20**

Internal grille for ventilation and air extraction.

Technical data

|  |  |
| --- | --- |
| Article: | IG 20 |
| Air direction: | Ventilation and air extraction |
| Loss of pressure: | 8 Pa |
| Installation: | Inside |
| Installation site: | Wall |
| Type of installation: | Surface-mounted |
| Material: | Synthetic material |
| Colour: | Pearl white, similar to RAL 1013 |
| Weight: | 0,18 kg |
| Weight including packaging: | 0,2 kg |
| Suitable for nominal size: | 200 mm |
| Width: | 258 mm |
| Height: | 258 mm |
| Depth: | 258 mm |
| Width with packaging: | 258 mm |
| Height with packaging: | 258 mm |
| Depth with packaging: | 258 mm |
| Ambient temperature: | 65 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799591719 |
| Article number: | 0059.0171 |

Manufacturer: MAICO

IG 20 Internal grille