**SGM 22**

Protective grille for fans in accordance with DIN EN ISO 13857.

Can be fitted on the inlet or pressure side.

SGM: Made of impact-resistant synthetic material, pearl white, similar to RAL 1013, for ERM duct fans.

SGM ... Ex: Made of metal for ERM-Ex fans, for use in areas subject to explosion hazards.

Technical data

|  |  |
| --- | --- |
| Article: | SGM 22 |
| Air direction: | Ventilation and air extraction |
| Material: | Synthetic material |
| Colour: | Pearl white, similar to RAL 1013 |
| Weight: | 0,012 kg |
| Weight including packaging: | 0 kg |
| Suitable for nominal size: | 224 mm |
| Width with packaging: | 230 mm |
| Height with packaging: | 30 mm |
| Depth with packaging: | 230 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799594284 |
| Article number: | 0059.0428 |

Manufacturer: MAICO

SGM 22