**Protective grille, metal SG 30**

Protective grille for fans in accordance with DIN EN ISO 13857.

Suitable for fans with duct connections.

Can be fitted on the inlet or pressure side.

Made of antistatic material, for use in areas subject to explosion hazards.

Technical data

|  |  |
| --- | --- |
| Article: | SG 30 |
| Air direction: | Ventilation and air extraction |
| Material: | Wire, chromated |
| Weight: | 0,49 kg |
| Weight including packaging: | 0,5 kg |
| Suitable for nominal size: | 300 mm |
| Width: | 369 mm |
| Height: | 369 mm |
| Depth: | 5,5 mm |
| Width with packaging: | 369 mm |
| Height with packaging: | 369 mm |
| Depth with packaging: | 270 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799501169 |
| Article number: | 0150.0116 |

Manufacturer: MAICO

SG 30 Protective grille, metal