**Fire protection compensation element BA 125/100-1**

Technical data

|  |  |
| --- | --- |
| Article: | BA 125/100-1 |
| Air direction: | Air extraction |
| Type of installation: | Recessed-mounted |
| Material: | Sheet steel |
| Weight: | 1,4 kg |
| Weight including packaging: | 1,42 kg |
| Fire protection: | yes |
| Number of couplings: | 1 |
| Suitable for nominal size: | 125 mm |
| Width: | 165 mm |
| Height: | 640 mm |
| Depth: | 125 mm |
| Width with packaging: | 165 mm |
| Height with packaging: | 640 mm |
| Depth with packaging: | 125 mm |
| Approval number: | Z-41.6-573 |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799990147 |
| Article number: | 0093.1008 |

Manufacturer: MAICO

BA 125/100-1 Fire protection compensation element