**FFU**

Flat channel system for controlled domestic ventilation.

Channel dimension: 110 mm x 54 mm.

Quick and easy installation.

Technical data

|  |  |
| --- | --- |
| Article: | FFU |
| Loss of pressure: | 2 Pa |
| Type of installation: | Recessed-mounted |
| Material: | Synthetic material |
| Synthetic material definition: | PVC-free polystyrene |
| Colour: | Pure white, similar to RAL 9010 |
| Weight: | 0,3 kg |
| Channel dimension: | 110 mm x 54 mm |
| Hydraulic diameter: | 72 mm |
| Width with packaging: | 115 mm |
| Height with packaging: | 280 mm |
| Depth with packaging: | 115 mm |
| Ambient temperature: | 60 °C |
| Packing unit: | 1 piece |
| Range: | D |
| GTIN (EAN): | 4012799520238 |
| Article number: | 0152.0023 |

Manufacturer: MAICO

FFU