**Ventilation duct coupling MT-Ü125**

For coupling between MT-R ventilation duct or MT-B ventilation elbow on ventilation ducts (e.g. folded spiral-seams ducts), units, wall and roof outlets.

Simple and reliable installation.

MT-Ü160/150: Can be used e.g. for couplings on folded spiral-seams ducts of nominal size 160 and 150.

Technical data

|  |  |
| --- | --- |
| Article: | MT-Ü125 |
| Model: | symmetrical |
| Material: | EPDM rubber |
| Weight: | 0,1 kg |
| Weight including packaging: | 0,11 kg |
| Nominal size: | 125 mm |
| Internal diameter: | 160 mm / 125 mm |
| External diameter: | 160 mm |
| Width: | 90 mm |
| Height: | 110 mm |
| Depth: | 80 mm |
| Width with packaging: | 90 mm |
| Height with packaging: | 110 mm |
| Depth with packaging: | 80 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799599869 |
| Article number: | 0059.0986 |

Manufacturer: MAICO

MT-Ü125 Ventilation duct coupling