**Ventilation duct coupling MT-Ü180**

For coupling between MT-R ventilation duct or MT-B ventilation elbow on ventilation ducts (e.g. folded spiral-seams ducts), units, wall and roof outlets.

Simple and reliable installation.

MT-Ü160/150: Can be used e.g. for couplings on folded spiral-seams ducts of nominal size 160 and 150.

Technical data

|  |  |
| --- | --- |
| Article: | MT-Ü180 |
| Model: | symmetrical |
| Material: | EPDM rubber |
| Weight: | 0,1 kg |
| Weight including packaging: | 0,13 kg |
| Nominal size: | 180 mm |
| Internal diameter: | 200 mm / 180 mm |
| External diameter: | 200 mm |
| Width: | 150 mm |
| Height: | 70 mm |
| Depth: | 70 mm |
| Width with packaging: | 150 mm |
| Height with packaging: | 70 mm |
| Depth with packaging: | 70 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799599890 |
| Article number: | 0059.0989 |

Manufacturer: MAICO

MT-Ü180 Ventilation duct coupling