**Radio switch DS RC**

EnOcean radio switch.

The radio switch can be used individually with the ECA ... ipro RC/RCH, ER 100 RC fans or the MAICOsmart system.

The radio switch can also be used in combination with the E-SM EnOcean plug-in module in order to control the WS 75 Powerbox, WS 120 Trio, WS 160 Flat, WS 170, WS 300 Flat, WS 320/470 and WR 310/410 centralised ventilation units using EnOcean.

For redevelopments and retrofit installations – no painting or wallpapering required.

Tiles don't need to be removed or renewed.

Use wherever no control cable can be installed.

Radio switch can be used on the move.

Radio switch requires no batteries.

Radio switch can be screwed on or glued to a glass surface.

Simple transmitter teaching-in saves on time-consuming programming.

Technical data

|  |  |
| --- | --- |
| Article: | DS RC |
| Battery: | not required |
| Degree of protection: | IP 20 |
| Mains cable: | not required |
| Installation site: | Wall |
| Type of installation: | Surface-mounted |
| Material: | Synthetic material |
| Colour: | Pure white, similar to RAL 9010 |
| Weight: | 0,07 kg |
| Weight including packaging: | 0,12 kg |
| Width: | 83 mm |
| Height: | 83 mm |
| Depth: | 16 mm |
| Width with packaging: | 87 mm |
| Height with packaging: | 87 mm |
| Depth with packaging: | 75 mm |
| Ambient temperature: | -25 °C up to 65 °C |
| Radio frequency: | 868,3 MHz |
| Number of radio channels: | 4 channels |
| Transmission range in the building: | 30 m |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799578321 |
| Article number: | 0157.0832 |

Manufacturer: MAICO

DS RC Radio switch