**Flexible aluminium duct AFR 125**

Flexible five-layered, grooved aluminium duct to be used as connecting duct to the main duct, in accordance with DIN 18017-3.

Non-combustible in accordance with DIN 4102 class A1 (building material classification).

Length details: extended length.

Technical data

|  |  |
| --- | --- |
| Article: | AFR 125 |
| Max. operating pressure: | 2.500 Pa |
| Material: | Aluminium |
| Weight: | 1,1 kg |
| Weight including packaging: | 1,24 kg |
| Suitable for nominal size: | 125 mm |
| Length: | 10 m |
| Width: | 10.000 mm |
| Height: | 135 mm |
| Depth: | 135 mm |
| Width with packaging: | 400 mm |
| Height with packaging: | 145 mm |
| Depth with packaging: | 145 mm |
| Ambient temperature: | 100 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799550914 |
| Article number: | 0055.0091 |

Manufacturer: MAICO

AFR 125 Flexible aluminium duct