**Disk valve, synthetic material TK 10**

Disk valves for ventilation and air extraction.

Sealed with a foam ring.

Linear air flow control via rotatable valve disk.

Easy installation with mounting ring and clamping springs.

Recommended accessories: FFE grease filter element for use in rooms where the exhaust air contains grease (e.g. kitchens etc.).

Technical data

|  |  |
| --- | --- |
| Article: | TK 10 |
| Air direction: | Ventilation and air extraction |
| Max. volumetric flow: | 30 m³/h |
| Material: | Synthetic material, antistatic |
| Colour: | Pure white, similar to RAL 9010 |
| Weight: | 0,13 kg |
| Weight including packaging: | 0,14 kg |
| Suitable for nominal size: | 100 mm |
| Width: | 150 mm |
| Height: | 150 mm |
| Depth: | 51 mm |
| Width with packaging: | 155 mm |
| Height with packaging: | 155 mm |
| Depth with packaging: | 70 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799511922 |
| Article number: | 0151.0192 |

Manufacturer: MAICO

TK 10 Disk valve, synthetic material