**Blower nozzle WD 10 D**

Blower nozzles for ventilation.

For ceiling installation.

With horizontal air outlet.

Linear air flow control by means of variable gaps.

Technical data

|  |  |
| --- | --- |
| Article: | WD 10 D |
| Air direction: | Ventilation |
| Max. volumetric flow: | 70 m³/h |
| Range of projection: | 5 m |
| Installation: | Inside |
| Installation site: | Ceiling |
| Material: | Sheet steel, powder coated |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 0,47 kg |
| Weight including packaging: | 0,49 kg |
| Suitable for nominal size: | 100 mm |
| Width: | 155 mm |
| Height: | 155 mm |
| Depth: | 81 mm |
| Width with packaging: | 156 mm |
| Height with packaging: | 156 mm |
| Depth with packaging: | 125 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799512912 |
| Article number: | 0151.0291 |

Manufacturer: MAICO

WD 10 D Blower nozzle