**Blower nozzle WD 10 W**

Blower nozzles for ventilation.

For wall mounting.

With horizontal air outlet.

Linear air flow control by means of variable gaps.

Technical data

|  |  |
| --- | --- |
| Article: | WD 10 W |
| Air direction: | Ventilation |
| Max. volumetric flow: | 45 m³/h |
| Range of projection: | 5 m |
| Installation: | Inside |
| Installation site: | Wall |
| Material: | Sheet steel, powder coated |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 0,43 kg |
| Weight including packaging: | 0,45 kg |
| Suitable for nominal size: | 100 mm |
| Width: | 130 mm |
| Height: | 142 mm |
| Depth: | 80 mm |
| Width with packaging: | 131 mm |
| Height with packaging: | 180 mm |
| Depth with packaging: | 140 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799512905 |
| Article number: | 0151.0290 |

Manufacturer: MAICO

WD 10 W Blower nozzle