**Tubular sound absorber RSR 40/50**

Tubular sound absorber for ventilation systems.

With sound absorbing cover made of synthetic resin-bonded glass fibres.

Non-combustible in accordance with DIN 4102 class A1 (building material classification).

Insertion loss measured in accordance with DIN 45646.

Temperature resistant up to +70 °C.

RSR...: With 25 mm thick sound absorption packing.

RSR.../50: With 50 mm thick sound absorption packing.

Technical data

|  |  |
| --- | --- |
| Article: | RSR 40/50 |
| Model: | 50 mm sound absorbing cover |
| Material: | Aluminium |
| Weight: | 4,4 kg |
| Weight including packaging: | 5,9 kg |
| Nominal size: | 400 mm |
| Width: | 513,5 mm |
| Height: | 513,5 mm |
| Depth: | 1.170 mm |
| Width with packaging: | 530 mm |
| Height with packaging: | 530 mm |
| Depth with packaging: | 1.180 mm |
| Insertion loss at 125 Hz: | 3 dB |
| Insertion loss at 250 Hz: | 6 dB |
| Insertion loss at 500 Hz: | 15 dB |
| Insertion loss at 1 kHz: | 18 dB |
| Insertion loss at 2 kHz: | 7 dB |
| Insertion loss at 4 kHz: | 6 dB |
| Insertion loss at 8 kHz: | 5 dB |
| Sound insulation: | yes |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799923367 |
| Article number: | 0092.0336 |

Manufacturer: MAICO

RSR 40/50 Tubular sound absorber