**Socket sound absorber SD 18**

Silencer for suction side sound insulation of roof fans.

With silencing elements made of abrasion-resistant and non-flammable mineral fibre plates.

Recommended accessories: SZ intermediate sockets for connecting ducts.

Technical data

|  |  |
| --- | --- |
| Article: | SD 18 |
| Max. flow velocity: | 20 m/s |
| Housing material: | Sheet steel, galvanised |
| Weight: | 25 kg |
| Weight including packaging: | 25 kg |
| Suitable for nominal size: | 180 mm |
| Width: | 765 mm |
| Height: | 850 mm |
| Depth: | 765 mm |
| Width with packaging: | 765 mm |
| Height with packaging: | 850 mm |
| Depth with packaging: | 765 mm |
| Insertion loss at 125 Hz: | 4 dB |
| Insertion loss at 250 Hz: | 10 dB |
| Insertion loss at 500 Hz: | 18 dB |
| Insertion loss at 1 kHz: | 22 dB |
| Insertion loss at 2 kHz: | 14 dB |
| Insertion loss at 4 kHz: | 15 dB |
| Total insertion loss: | 15 dB |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799923374 |
| Article number: | 0092.0337 |

Manufacturer: MAICO

SD 18 Socket sound absorber