**Heat exchanger WT 300**

Heat exchanger for heat recovery in ventilation systems.

Can be combined with an additional bypass module for winter or summer operation.

With condensation drainage - diameter approx. 13 mm.

Safety instructions

Combination with MAICO TH 10 thermostat for frost protection is recommended.

Technical data

|  |  |
| --- | --- |
| Article: | WT 300 |
| Installation site: | Channel |
| Material: | EPS |
| Weight: | 7,9 kg |
| Weight including packaging: | 10,05 kg |
| Nominal size: | 160 mm |
| Width: | 550 mm |
| Height: | 508 mm |
| Depth: | 690 mm |
| Width with packaging: | 710 mm |
| Height with packaging: | 465 mm |
| Depth with packaging: | 570 mm |
| Ambient temperature: | 40 °C |
| Heat exchanger construction type: | Cross flow |
| Packing unit: | 1 piece |
| Range: | D |
| GTIN (EAN): | 4012799520207 |
| Article number: | 0152.0020 |

Manufacturer: MAICO

WT 300 Heat exchanger