**Water air heater WRH 20-2**

Water air heater for ventilation systems.

Connections made of copper.

Housing cover can be removed for service work.

With rubber seal on the air connection couplings.

Technical data

|  |  |
| --- | --- |
| Article: | WRH 20-2 |
| Installation position: | vertical / horizontal |
| Housing material: | Sheet steel, galvanised |
| Weight: | 5,23 kg |
| Weight including packaging: | 5,61 kg |
| Nominal size: | 200 mm |
| Open cross section: | 1.701 cm² |
| Width: | 305 mm |
| Height: | 258 mm |
| Depth: | 380 mm |
| Width with packaging: | 375 mm |
| Height with packaging: | 285 mm |
| Depth with packaging: | 381 mm |
| Air heater type: | Water |
| Heater power rating: | 5.000 W |
| Mass flow: | 210 kg/h |
| Inlet temperature: | 70 °C |
| Return flow temperature: | 50 °C |
| Max. water temperature: | 100 °C |
| Max. water pressure: | 6 bar |
| Water pressure difference: | 11.100 Pa |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799821199 |
| Article number: | 0082.0119 |

Manufacturer: MAICO

WRH 20-2 Water air heater