**Water air heater WRH 40-9**

Water air heater for ventilation systems.

Connections made of copper.

Housing cover can be removed for service work.

With rubber seal on the air connection couplings.

Technical data

|  |  |
| --- | --- |
| Article: | WRH 40-9 |
| Installation position: | vertical / horizontal |
| Housing material: | Sheet steel, galvanised |
| Weight: | 12,99 kg |
| Weight including packaging: | 13,83 kg |
| Nominal size: | 400 mm |
| Open cross section: | 4.050 cm² |
| Width: | 540 mm |
| Height: | 483 mm |
| Depth: | 440 mm |
| Width with packaging: | 530 mm |
| Height with packaging: | 430 mm |
| Depth with packaging: | 590 mm |
| Air heater type: | Water |
| Heater power rating: | 20.600 W |
| Mass flow: | 850 kg/h |
| Inlet temperature: | 70 °C |
| Return flow temperature: | 50 °C |
| Max. water temperature: | 100 °C |
| Max. water pressure: | 6 bar |
| Water pressure difference: | 8.300 Pa |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799821229 |
| Article number: | 0082.0122 |

Manufacturer: MAICO

WRH 40-9 Water air heater