**Intermediate socket SZ 22**

Intermediate sockets for roof fans.

For a connection between the SD socket sound absorber and the ventilation ducts that is economical in terms of air flow and easy to mount.

For installation in flat roofs.

Technical data

|  |  |
| --- | --- |
| Article: | SZ 22 |
| Installation site: | Roof |
| Housing material: | Sheet steel, galvanised |
| Weight: | 6,8 kg |
| Weight including packaging: | 6,82 kg |
| Suitable for nominal size: | 225 mm |
| Width: | 800 mm |
| Height: | 800 mm |
| Depth: | 180 mm |
| Width with packaging: | 800 mm |
| Height with packaging: | 800 mm |
| Depth with packaging: | 180 mm |
| Ambient temperature: | 100 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799922872 |
| Article number: | 0092.0287 |

Manufacturer: MAICO

SZ 22 Intermediate socket