**Fixing cuff ELR 35**

Fixing cuffs for sound and vibration dampening of duct fans.

With 10 mm thick neoprene coating.

Technical data

|  |  |
| --- | --- |
| Article: | ELR 35 |
| Material: | Sheet steel, galvanised |
| Weight: | 0,4 kg |
| Weight including packaging: | 0,44 kg |
| Suitable for nominal size: | 350 mm |
| Width: | 377 mm |
| Height: | 377 mm |
| Depth: | 60 mm |
| Width with packaging: | 377 mm |
| Height with packaging: | 377 mm |
| Depth with packaging: | 60 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799921158 |
| Article number: | 0092.0115 |

Manufacturer: MAICO

ELR 35 Fixing cuff