**Counter socket GS 45**

Counter socket for fitting flexible cuffs on ventilation ducts.

Suited to assembly of folded spiral-seams duct in combination with EL / EL Ex flexible cuffs only.

Technical data

|  |  |
| --- | --- |
| Article: | GS 45 |
| Material: | Sheet steel, galvanised |
| Weight: | 0,86 kg |
| Weight including packaging: | 0,9 kg |
| Suitable for nominal size cuffs: | 450 mm |
| Width: | 512 mm |
| Height: | 512 mm |
| Depth: | 50 mm |
| Width with packaging: | 512 mm |
| Height with packaging: | 512 mm |
| Depth with packaging: | 50 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799551737 |
| Article number: | 0055.0173 |

Manufacturer: MAICO

GS 45 Counter socket