**Mounting foot FUR 16S/20/25**

Mounting feet for the assembly of ERR fans on walls, ceilings or brackets.

Technical data

|  |  |
| --- | --- |
| Article: | FUR 16S/20/25 |
| Installation site: | Wall / Ceiling |
| Material: | Sheet steel, galvanised |
| Weight: | 0,47 kg |
| Weight including packaging: | 0,49 kg |
| Suitable for nominal size: | 160 mm / 200 mm / 250 mm |
| Width: | 395 mm |
| Height: | 83 mm |
| Depth: | 80 mm |
| Width with packaging: | 220 mm |
| Height with packaging: | 40 mm |
| Depth with packaging: | 90 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799360889 |
| Article number: | 0036.0088 |

Manufacturer: MAICO

FUR 16S/20/25 Mounting foot