**Masking frame ER-AR**

Masking frame for all ER-UP... housings.

Covers joints between the recessed housing and the wall tiles.

Prevents unattractive gaps around the recessed housing.

Scope of delivery:

Masking frame

Fixing screw.

Technical data

|  |  |
| --- | --- |
| Article: | ER-AR |
| Installation: | Inside |
| Type of installation: | Surface-mounted |
| Material: | Synthetic material |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 0,21 kg |
| Weight including packaging: | 0,22 kg |
| Width: | 280 mm |
| Height: | 280 mm |
| Depth: | 50 mm |
| Width with packaging: | 281 mm |
| Height with packaging: | 281 mm |
| Depth with packaging: | 51 mm |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799598992 |
| Article number: | 0059.0899 |

Manufacturer: MAICO

ER-AR Masking frame