**Spacing frame DR 60/100**

Spacing frame for ER-UP.. recessed-mounted housings that have not been plastered deep enough.

Maximum depth: 20 mm.

Fit a spacing frame between the wall and the internal cover.

Technical data

|  |  |
| --- | --- |
| Article: | DR 60/100 |
| Type of installation: | Surface-mounted |
| Material: | Synthetic material |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 0,11 kg |
| Weight including packaging: | 0,11 kg |
| Width: | 253 mm |
| Height: | 253 mm |
| Depth: | 30 mm |
| Width with packaging: | 254 mm |
| Height with packaging: | 254 mm |
| Depth with packaging: | 31 mm |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799599289 |
| Article number: | 0059.0928 |

Manufacturer: MAICO

DR 60/100 Spacing frame