**Wall frame ER-MR**

Wall frames for housings that have been plastered too deep, to prevent the air from being drawn out of the shaft.

Can be combined with all ER-UP... housings.

Consists of 2 plate frames that can be slid inside each other.

Adjustable depth: 60 mm to 90 mm.

With 100 mm long screw.

Technical data

|  |  |
| --- | --- |
| Article: | ER-MR |
| Type of installation: | Recessed-mounted |
| Material: | Sheet steel, galvanised |
| Colour: | Silver |
| Weight: | 0,79 kg |
| Weight including packaging: | 0,8 kg |
| Width: | 230 mm |
| Height: | 230 mm |
| Depth: | 60 mm |
| Width with packaging: | 230 mm |
| Height with packaging: | 230 mm |
| Depth with packaging: | 60 mm |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799180241 |
| Article number: | 0018.0024 |

Manufacturer: MAICO

ER-MR Wall frame