**Air extraction socket ER-AS**

Extraction sockets for ER GH, ER GH-VWR, ER-UPD and ER-UP/G flush-mounted housing for toilet seat air extraction. Air extraction of room and WC seat at the same time.

Pre-requirements: The flushing pipe from the recessed-mounted toilet cistern is fitted with a DN 70 branch.

Connection from flushing pipe to the HT DN 70 fan, resulting in reduced air speeds and effective, draught-free extraction.

Combination with ER EC, ER 60 or ER 100.

Cistern recommendation: Manufacturer TECE, TECEprofil Universal module for WC with TECE cistern with connection for odour extraction. TECE Order no.: 9.300.003, www.tece.de, Tel.: +49 (0) 25 72 / 928-0

Technical data

|  |  |
| --- | --- |
| Article: | ER-AS |
| Air direction: | Air extraction |
| Installation site: | Wall |
| Material: | Synthetic material |
| Colour: | Black |
| Weight: | 0,06 kg |
| Weight including packaging: | 0,1 kg |
| Width: | 83 mm |
| Height: | 83 mm |
| Depth: | 80 mm |
| Width with packaging: | 155 mm |
| Height with packaging: | 155 mm |
| Depth with packaging: | 125 mm |
| Ambient temperature: | 60 °C |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799939283 |
| Article number: | 0093.0928 |

Manufacturer: MAICO

ER-AS Air extraction socket