**Pressure controller Centro-PT**

Centro-PT: With integrated pressure cell and timer .

Features

Can be used with MAICO Centro centralised ventilation system.

Automatic control of the negative pressure at different operating states.

The motor voltage is controlled steplessly through phase angles.

Only for single-phase asynchronous motors, ESR 16-2 to ESR 40-2 sound-insulated ventilation box.

Robust plastic housing.

With see-through lid and terminal box.

Green LED display: Ready for operation.

Red LED display: Fault.

Display of the current pressure value.

Display of the motor voltage.

With on/off switch.

Technical data

|  |  |
| --- | --- |
| Article: | Centro-PT |
| Control unit rated voltage: | 230 V |
| Maximum load: | 8 A |
| Degree of protection: | IP 54 |
| Fan mains cable: | 3 x 1,5 mm² |
| Fan with motor protection mains cable: | 5 x 1,5 mm² |
| Mains cable control: | 3 x 1,5 mm² |
| Pressure cell feed: | 2 x 2 x 0.6 |
| Voltage at the output: | 0 - 230 V |
| Installation site: | Wall |
| Housing material: | Synthetic material |
| Colour: | Light grey |
| Weight: | 1,5 kg |
| Weight including packaging: | 1,82 kg |
| Width: | 220 mm |
| Height: | 190 mm |
| Depth: | 110 mm |
| Width with packaging: | 275 mm |
| Height with packaging: | 200 mm |
| Depth with packaging: | 140 mm |
| Ambient temperature: | 40 °C |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799573999 |
| Article number: | 0157.0399 |

Manufacturer: MAICO

Centro-PT Pressure controller