**Air filter TFE 40-5**

Air filter for ventilation systems.

Inspection lid can be removed for easy filter exchange.

With synthetic fibre filter insert.

Panel filter.

Filter insert not regenerable.

With rubber sealing ring on the air connection sockets.

TFE ...-5: Filter class F5, accessories for replacement filter RF...-5

TFE ...-7: Filter class ISO ePM1 50 % (F7), accessories for replacement filter RF...-7

Recommended accessories: DW 1000 differential pressure controller.

Installation instructions

Monitor filter resistance using DW 1000 differential pressure controller.

Technical data

|  |  |
| --- | --- |
| Article: | TFE 40-5 |
| Installation position: | vertical / horizontal |
| Housing material: | Sheet steel, galvanised |
| Weight: | 8,73 kg |
| Weight including packaging: | 10,68 kg |
| Filter class: | F5 |
| Nominal size: | 400 mm |
| Width: | 560 mm |
| Height: | 530 mm |
| Depth: | 300 mm |
| Width with packaging: | 800 mm |
| Height with packaging: | 610 mm |
| Depth with packaging: | 410 mm |
| Ambient temperature: | 80 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799490661 |
| Article number: | 0149.0066 |

Manufacturer: MAICO

TFE 40-5 Air filter