**Air filter, replacement RF 10/16-5**

Replacement filter for TFE air filter.

RF ...-5: Replacement filter for TFE...-5.

RF ...-7: Replacement filter for TFE...-7.

Technical data

|  |  |
| --- | --- |
| Article: | RF 10/16-5 |
| Installation position: | vertical / horizontal |
| Weight: | 0,31 kg |
| Weight including packaging: | 0,6 kg |
| Filter class: | ISO ePM10 60 % (F5) |
| Nominal size in mm: | 100-160 |
| Width: | 288 mm |
| Height: | 288 mm |
| Depth: | 28 mm |
| Width with packaging: | 288 mm |
| Height with packaging: | 288 mm |
| Depth with packaging: | 28 mm |
| Ambient temperature: | 80 °C |
| Packing unit: | 2 pieces |
| Range: | C |
| GTIN (EAN): | 4012799938750 |
| Article number: | 0093.0875 |

Manufacturer: MAICO

RF 10/16-5 Air filter, replacement