**Potentiometer ST EC 3**

Potentiometer for controlling EC fans.

Output voltage for ST EC 10 and ST EC 230 can be set in continuously variable manner between 0 - 10 V using rotary knob.

ST EC 3 permits regulation of output voltage over 3 levels:

Level 1 = 3 - 7 V can be set

Level 2 = 5 - 9 V can be set

Level 3 = 10 V

The potentiometer can be fitted in both a recessed-mounted box without housing (IP 44) and surface-mounted with the housing (IP 54).

Additional switching contact for ST EC 010 permits e.g. a controller release to be connected.

ST EC 230 for connection to a 230 V power supply.

ST EC 010 for connection to a 10 V power supply.

ST EC 3 for connection to a 10 - 15 V power supply.

Technical data

|  |  |
| --- | --- |
| Article: | ST EC 3 |
| Type of voltage: | Direct current |
| Rated voltage: | 10 V - 15 V |
| Output signal: | 0 V - 10 V |
| Degree of protection: | IP 54 |
| Type of installation: | Surface-mounted / Recessed-mounted |
| Housing material: | Synthetic material |
| Colour: | Pure white, similar to RAL 9010 |
| Weight: | 0,14 kg |
| Weight including packaging: | 0,16 kg |
| Width: | 82 mm |
| Height: | 82 mm |
| Depth: | 65 mm |
| Width with packaging: | 95 mm |
| Height with packaging: | 85 mm |
| Depth with packaging: | 70 mm |
| Packing unit: | 1 piece |
| Range: | E |
| GTIN (EAN): | 4012799571117 |
| Article number: | 0157.0111 |

Manufacturer: MAICO

ST EC 3 Potentiometer