**Speed controller ST 5**

Speed controller for linear control of the fans.

Minimum speed adjustable.

Function principle: Phase angle control.

Recommended distance from radios and televisions: 3 m.

Switch on the fans at maximum speed by turning the knob. Turning further reduces the speed.

Splash water protected.

With operating indicator light.

VDE-tested.

Additional switching contact (230 V) e.g. for controlling a shutter.

There can be a physically induced humming noise at lower speeds, through the use of phase angle technology. TRE... 5-step transformers are therefore used for speed control in rooms requiring quiet fan operations.

Assembly on walls possible; avoid ceiling installation because of temperature build-up.

Technical data

|  |  |
| --- | --- |
| Article: | ST 5 |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Maximum load: | 4,3 A |
| Minimum load: | 0,2 A |
| Degree of protection: | IP 44 |
| Type of installation: | Surface-mounted |
| Colour: | Pure white, similar to RAL 9010 |
| Weight: | 0,5 kg |
| Weight including packaging: | 0,54 kg |
| Width: | 85 mm |
| Height: | 170 mm |
| Depth: | 63 mm |
| Width with packaging: | 95 mm |
| Height with packaging: | 185 mm |
| Depth with packaging: | 80 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799578123 |
| Article number: | 0157.0812 |

Manufacturer: MAICO

ST 5 Speed controller