**Reversing switch UWK 1**

Reversing switch for ventilation and air extraction.

With masking frame for combination with STU 1 or STU 2.5.

Technical data

|  |  |
| --- | --- |
| Article: | UWK 1 |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Frequency: | 50 Hz/60 Hz |
| Imax: | 1 A |
| Type of installation: | Recessed-mounted |
| Colour: | Alpine white |
| Weight: | 0,1 kg |
| Weight including packaging: | 0,14 kg |
| Width: | 80 mm |
| Height: | 150 mm |
| Depth: | 10 mm |
| Width with packaging: | 85 mm |
| Height with packaging: | 190 mm |
| Depth with packaging: | 58 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799578178 |
| Article number: | 0157.0817 |

Manufacturer: MAICO

UWK 1 Reversing switch