**Speed controller, reversing switch STW 1**

For air extraction and ventilation.

With operating indicator light.

VDE-tested.

Additional switching contact (230 V) e.g. for controlling a shutter.

There can be a physically induced humming noise at lower speeds, through the use of phase angle technology. TRE... 5-step transformers are therefore used for speed control in rooms requiring quiet fan operations.

Technical data

|  |  |
| --- | --- |
| Article: | STW 1 |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Maximum load: | 1 A |
| Minimum load: | 0,1 A |
| Degree of protection: | IP 20 |
| Type of installation: | Surface-mounted |
| Colour: | Pearl white, similar to RAL 1013 |
| Weight: | 0,26 kg |
| Weight including packaging: | 0,3 kg |
| Width: | 128 mm |
| Height: | 74 mm |
| Depth: | 54 mm |
| Width with packaging: | 145 mm |
| Height with packaging: | 77 mm |
| Depth with packaging: | 60 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799578130 |
| Article number: | 0157.0813 |

Manufacturer: MAICO

STW 1 Speed controller, reversing switch