**5-step switch for TRE...S -2/ TR...S-2 5-step transformers ESS 20**

5-step switch for TRE...S-2 and TR...S-2 5-step transformers.

For front-mounting in the control cabinet.

ESS: Accessories for AC fans.

DSS: Accessories for three-phase AC fans.

Technical data

|  |  |
| --- | --- |
| Article: | ESS 20 |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Frequency: | 50 Hz/60 Hz |
| Maximum load: | 20 A |
| Degree of protection: | IP 00 |
| Type of installation: | Control cabinet |
| Weight: | 0,16 kg |
| Weight including packaging: | 0,19 kg |
| Width: | 72 mm |
| Height: | 72 mm |
| Depth: | 81 mm |
| Width with packaging: | 95 mm |
| Height with packaging: | 85 mm |
| Depth with packaging: | 85 mm |
| Ambient temperature: | 0 °C up to 40 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799577492 |
| Article number: | 0157.0749 |

Manufacturer: MAICO

ESS 20 5-step switch for TRE...S -2/ TR...S-2 5-step transformers