**Interval switch VZI 10**

Interval switch for regular ventilation of rarely used rooms.

Fan can be switched on via interval switch and via manual operation.

Can be operated via commercially available switches.

Interval time adjustable: 1 h 15 h.

Mounting in flush-mounted box possible.

Technical data

|  |  |
| --- | --- |
| Article: | VZI 10 |
| Rated voltage: | 230 V |
| Frequency: | 50 Hz/60 Hz |
| Maximum load: | 1,25 A |
| Degree of protection: | IP 40 |
| Weight: | 0,01 kg |
| Weight including packaging: | 0,02 kg |
| Width: | 20 mm |
| Height: | 13 mm |
| Depth: | 35 mm |
| Width with packaging: | 20 mm |
| Height with packaging: | 13 mm |
| Depth with packaging: | 35 mm |
| Ambient temperature: | 0 °C up to 50 °C |
| Remote control: | - |
| Overrun time: | 10 min |
| Switch-on duration: | 10 min |
| Start delay: | 50 s |
| Packing unit: | 1 piece |
| Range: | A |
| GTIN (EAN): | 4012799578239 |
| Article number: | 0157.0823 |

Manufacturer: MAICO

VZI 10 Interval switch