**Temperature control system DTL 24 P**

Electronic temperature controller for controlling the DHP electrical air heater.

Night reduction can be set from 0 K to 4 K below the setpoint temperature.

Triac regulator with pulse packet control.

Control via 0 V to 10 V possible.

To increase power up to 30 kW, use DTL 2 P-L.

Technical data

|  |  |
| --- | --- |
| Article: | DTL 24 P |
| Type of voltage: | Three-phase AC |
| Rated voltage: | 400 V |
| PMax: | 16.500 W |
| Maximum load: | 24 A |
| Degree of protection: | IP 20 |
| Type of installation: | Surface-mounted |
| Weight: | 1,65 kg |
| Weight including packaging: | 1,78 kg |
| Width: | 200 mm |
| Height: | 290 mm |
| Depth: | 195 mm |
| Width with packaging: | 180 mm |
| Height with packaging: | 220 mm |
| Depth with packaging: | 95 mm |
| Packing unit: | 1 piece |
| Range: | D |
| GTIN (EAN): | 4012799575863 |
| Article number: | 0157.0586 |

Manufacturer: MAICO

DTL 24 P Temperature control system